Router configuration – R0

- Design network connection

enable

configure terminal

interface FastEthernet 0/0

ip address 10.163.0.254 255.255.255.0

no shutdown

end

write

- Marketing network connection

config terminal

interface FastEthernet 1/0

ip address 10.163.1.254 255.255.255.0

no shutdown

end

write

-DHCP configuration

Vai ser criada uma pool para cada network

Design:

enable

config terminal

service dhcp

ip dhcp pool designPool

network 10.163.0.0 255.255.255.0

default-router 10.163.0.254

Marketing:

config terminal

service dhcp

ip dhcp pool mPool

network 10.163.1.0 255.255.255.0

default-router 10.163.1.254